--- a/dmx_usb.c
+++ b/dmx_usb.c
@@ -20,7 +20,7 @@
 #include <linux/module.h>
 #include <linux/spinlock.h>
 #include <linux/completion.h>
-#include <asm/uaccess.h>
+#include <linux/uaccess.h>
 #include <linux/usb.h>
 #include <linux/version.h>
 
